Resilient-seated gate valve to EN 13774 
For gases according to DVGW Guideline G 260
Shut-off valve for gas systems and gas pipelines up to 50° C
DN 50 - 200, PN 16
With PE-HD ends to SDR 11 on both sides

Rubber-coated shut-off wedge with sliding caps to reduce wear and tear and operation torques, which increases the service life;
Significantly lower actuation torques than EN 1072-2 requirement
Maintenance-free and corrosion-resistant extended stem seal with triple O ring sealing located in the bush;
Designed for butt welding and arc welding of sockets, length for two times welding possible;
Body, cover and wedge made of ductile cast iron EN-JS 1030 (GGG-40);
PE-HD ends: PE 100;
Wedge NBR rubber coated on all sides;
Stem made of stainless steel grade 431;
Final inspection test to EN 12266 (DIN 3230 Part 5 PG3)
With integrated adapter for the TELEMAX® stem extension

Corrosion protection:
Inside and outside epoxy coated in GSK type “heavy-duty corrosion protection” to 
DIN 30 677-2, coating thickness >250 µm, colour: yellow

VAG EKO®plus PE Gate Valve - gas or equivalent

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
- with handwheel
- with stem square cap
- with surface box
- with support plate

Quantity ........    €/piece ........    €/item .......