Metallic sealing gate valve to EN 1171 (DIN 3352, Part 2)
Non-rising stem
Shut-off valve for waste water
DN 50 - 1200, PN 10
Face-to-face length DIN EN 558-1, basic series 15 (DIN 3202, F5)

With handwheel;
Readjustable stem seal with stuffing box;
With threaded drain plug;
Flange connection dimensions to EN 1092-2; PN 10;
Body, bonnet and wedge made of ductile cast iron EN-JS 1030 (GGG-40);
Body- and wedge seat rings made of zinc-free bronze (waste-water resistant);
Stem made of waste water resistant stainless steel grade 1.4057;
Stem nut made of zinc-free bronze (waste-water resistant);
Bonnet screws and washers made of stainless steel grade 316

Corrosion protection:
Inside and outside epoxy coated, coating thickness 250 µm, colour: RAL 5005 blue

VAG KOS Gate Valve KAT 1130 
or equivalent

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
- with gear unit
- with mechanical position indicator
- prepared for electric actuator
- with O ring seal for buried installation
- with stem extension
- with bypass 
- DN 50 - 600, PN 16 

Quantity ........    €/piece ........    €/item .......