Metallic sealing gate valve to EN 1171 
Non rising stem
Shut-off valve for service water up to 200° C
DN 40 - 300, PN 10 - 16
Face-to-face length DIN EN 558-1, basic series 15 (DIN 3202, F5)

Maintenance-free and corrosion-resistant stem sealing;
O ring seal;
Flange connection dimensions to EN 1092-2;
Body, cover and wedge made of cast iron EN-JL 1040 (GG-25);
Body- and wedge seat rings made of stainless steel grade 304;
Stem made of stainless steel grade 304;
O rings made of Viton

Corrosion protection:
Inside and outside with liquid synthetic resin coating, colour: RAL 6011 green

VAG IKO®plus Gate Valve or equivalent	

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
- with handwheel
- with SERIO®plus position indicator
- with drain plug
- body- and wedge seat rings made of brass / O rings made of EPDM (150° C)

Quantity ........    €/piece ........    €/item .......