Underground hydrant with double shut-off 
Type AD to EN 1074-6 and EN 14339
DIN-DVGW registered for drinking water
DN 100, PN 16

Automatic ball shut-off
Double draining system with two independent drain ports with pressure water protection – no remaining water after closing the hydrant;
With integrated safety interlock of the main valve assembly;
Claw with self-closing cover, claw DN 100 with retaining lugs;
Enclosed, backlash-free stem bearing;
Maintenance-free stem seal with triple O ring seal in a brass bushing;
Integrated multi-functional seal at the connection flange;
Flange connection dimensions to EN 1092-2;
All parts in touch with the fluid to KTW and DVGW Code of Practice W270 (no build-up of harmful bacteria);
Jacket, cap and claw made of ductile cast iron;
Valve cone made of ductile cast iron fully vulcanised with EPDM;
Stem made of stainless steel grade 420;
All bolts made of stainless steel A2;
Pressure pipe and connecting pins made of stainless steel grade 304;

Corrosion protection
Inside and outside epoxy coated in GSK type “heavy-duty corrosion protection” to 
DIN 30 677-2, coating thickness >250 µm, colour: RAL 5005 blue

VAG HYDRUS® G2 DN 100 Underground Hydrant, Type AD or equivalent	

Cover depth: 1.00 m, 1.25 m or 1.50 m

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Variety:
-Claw DN 80 with retaining lug

Quantity.......    €/Piece.......    €/Item......