Underground hydrant for low depth 
DN 65, PN 10 (Trommelbohrung)

Maintenance-free stem seal;
Body parts made of ductile cast iron GGG-40;
Stem made of stainless steel grade 420;
Valve cone made of ductile cast iron, vulcanised with EPDM;
Flange connection dimensions according to the Württemberg specification;
Bolts with nuts made of stainless steel type grade A2

Corrosion protection:	
Inside and outside epoxy coated, colour: RAL 5005 blue

VAG Hydrant for Low Depth or equivalent

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
- right-hand closing with flange to DIN EN 1092
- with automatic draining 

Quantity ........    €/piece ........    €/item .......