Tapping bridge
DN 80 - 200, PN 16

Self-drilling with integrated hollow drill
Easy tapping under pressure without tapping machine or auxiliary shut-off-device
With outlet female-thread connection G 1½ ;
Top-drilling under pressure from
	- PVC pipes (maximum wall thickness 12 mm)
	- PE-HD- pipes (maximum  wall thickness 14.6 mm)
Tapping diameter: DN 80…100=27 mm; DN 125…200=38 mm
The integrated brass hollow drill is used as main isolation after drilling;
Limit stop and clamp made of ductile iron EN-JS 1030 (GGG-40);
With unlosable EPDM-elastomer seal strip; Clearly separated sealing and holding function;
All parts in touch with the fluid to KTW and DVGW Code of Practice W270 (no build-up of harmful bacteria);
Nickel-plated brass angle valve;
Stainless-steel drive shaft 
Connection screws, nuts and disks stainless-steel A 2 quality 
with PE-HD protective caps;

Corrosion protection: 
Limit stop and clamp: inside and outside epoxy coated in GSK type “heavy-duty corrosion protection” to 
DIN 30 677-2, coating thickness >250 µm, colour: RAL 5005 blue

VAG Tapping bridge TERRA® K1 or equivalent	

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
-	transition piece for PE-HD house connections Da 32/40/50
-	TERRA®lock thread-adapter for TERRA®lock -fitting-connection

Quantity ........    €/piece ........    €/item .......