Automatic air valve, single-chamber type
Air valve for drinking and service water up to 50°C
DN 25, PN 16
with female thread connection G ¾ / G 1 / G 1¼

Single-chamber valve directly operated by the medium;
Minimum pressure required for perfect sealing capacity: 0.5 bar;
Two-level venting system with 3 functions (supply and release of air as well as automatic air release during operation); 
Connection thread to DIN ISO 228-1 for attaching to the pipeline;
Body and cap made of ductile cast iron EN-JS 1030 (GGG-40);
Float made of plastic

Corrosion protection:
Inside and outside with epoxy coating to GSK standards for heavy-duty corrosion protection
to DIN 30 677-2, coating thickness >250 µm, colour: RAL 5005 blue

VAG BEV-E Automatic Air Valve or equivalent	

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Varieties:
- with ¾“ connection thread 
- with 1 ¼“ connection thread 
- with ball valve as shut-off valve 
- nominal pressure PN 25

Quantity ........    €/piece ........    €/item .......