Control Valve, Float operated
PN 10 - 16
DN 40 - 150
soft sealing
face-to-face to EN 558-1, series 1, (DIN 3202, F1),
body and bonnet of ductile iron EN-JS 1030 (GGG-40),
flange dimensions to DIN EN 1092, PN 10/16
with pressure balanced valve piston,
with slotted regulation cylinder for linear regulating characteristic,
internals of corrosion resistant material,
with lever, in stainless steel
float of stainless steel
Corrosion protection:	inside and outside
epoxy coating,
blue, RAL 5005

Flange connection dimensions acc. DIN EN 1092,

design data:
Q max. ... m 3/h    Q min. ... m 3/h
upstream pressure at Q max. ... bar, at Q min. ... bar
downstream pressure at Q max. ...bar, at Q min. ...bar

e.g.  VAG DURA Float Valve or equivalent	

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Pcs. ..... Euro/pcs.....    Euro/item.....