EN-part (Hydrant bend) acc. EN 545
PN 16
DN 80...100

Horizontal connection with double-function socket for positive, direct interior interlocking 
With BAIO®plus System parts and for exterior interlocking of cast-iron and plastic pipes;
Socket designed for sealing ring to DIN 28 603;
Vertical connection designed as flange connection;
Flange connection dimensions to DIN EN 1092;
Can be supplied with three G 1½ outlets on the sides;
Made of ductile iron EN-JS 1030 (GGG-40);

Corrosion protection:
Inside and outside epoxy-coated with GSK type “heavy-duty corrosion protection” to
DIN 30 677-2, coating thickness >250 µm, colour: RAL 5005 blue
		
VAG BAIO®EN-part or equivalent

Manufacturer:	VAG GmbH
		Carl-Reuther-Str. 1	
		68305 Mannheim
		Germany
		www.vag-group.com

Quantity ........    €/piece ........    €/item. .......